# Adafruit SHT31-D Temperature and Humidity Sensor Breakout [![Build Status](https://github.com/adafruit/Adafruit_SHT31/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_SHT31/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_SHT31/html/index.html)

<a href="https://www.adafruit.com/product/2857"><img src="assets/board.jpg?raw=true" width="500px"></a>

This is a library for the SHT31 Digital Humidity + Temp sensor.

It is designed specifically to work with the SHT31 Digital in the Adafruit shop:

* https://www.adafruit.com/products/2857

These sensors use **I2C** to communicate, 2 pins are required to interface

Adafruit invests time and resources providing this open source code,
please support Adafruit and open-source hardware by purchasing
products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.  
BSD license, all text above must be included in any redistribution

Check out the links above for our tutorials and wiring diagrams

## Installation

Use the Arduino Library Manager to install this library. If you're unfamiliar
with how this works, we have a great tutorial on Arduino library installation
at: http://learn.adafruit.com/adafruit-all-about-arduino-libraries-install-use
